Exercises 4

LLSMF2018\_ELEC

1. Download the project included in "interrupts.zip".
2. Program your board (the LCD screen still attached to JC and JD connectors).

* Try to push button 1 and 2.
* Look at the code. Notice that the two interrupts have 2 different frequencies.
* How is button1 handled? How do we detect a single push?

1. Rewrite previous exercises (Exercise sessions 2 & 3) taking benefit of the new possibilities offered by the interrupts.